BusinessPhone Communication Platform 6.0
Commands > Commands 8000...8999

## 8019
Wake-up order time 2

A guest who orders a wake-up call from a telephone without display will receive a voice message as acknowledgement.

Wake-up acknowledgements can be supplied in three different languages.

With commands 8009 Wake-up language 1-8011 Wake-up language 3 the three languages in which wake-up-messages can be given are stated. Commands 8015 Wake-up order ref 1-8017 Wake-up order ref 3 are used to determine the wake-up acknowledgements to be supplied for the respective language.

Commands 8018 Wake-up order time 1-8020 Wake-up order time 3 are used to determine whether the ordered wake-up time shall also be included in the wake-up acknowledgement.

This command is used to determine whether the wake-up time shall be included in the wake-up acknowledgement for the 2nd language.

Commands 4407 Hours – language 2 and 4408 5 Minutes interval – language 2 are used to program the wake-up times for the 2nd language.

##### Valid data

Yes |  |  |
No |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2004