BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0x88
Undefined Ringsignal

Default definition: |  | ERROR + TRIG |
Used by block: |  | EX |
Category: |  | DESIGNER |

The terminator head, which indirectly indicates which ring signal should be used towards an extension, was invalid.

- D1: The invalid terminator head.
- D2: Current process state.
- D3: Undefined
- D4: Undefined

Revision: I © Ericsson Enterprise 2004