BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1104
Reroute position at night

This command is used to determine the rerouting position for the trunk in a night-switched exchange. This is the position to which unanswered external calls, e.g. parked calls, camped-on calls and transfer before answer, are routed. The rerouting position is determined by stating its directory number. The individual extension is removed by blanking out the current directory number.

If there is no rerouting position, the trunk will be parked for general access. The call will also be presented on all system telephones on which the trunk is represented by a function key.

The rerouting position is selected by stating its directory number. Erasure of the directory number results in erasure of the rerouting position.

The call will be presented on system telephones where the trunk is represented by a key.

Note

If the individual answering position and the rerouting position are removed for the trunk, ensure that the trunk is represented on a function key so that incoming calls can be presented.

Therefore please check commands 1102 Answering position at night, 1407 Maximum hold time and command group 03.

##### Valid data

0-4 |  | characters (0-9,*,#) |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004