BusinessPhone Communication Platform 6.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## BB VMCTRL

10h VMPLAY |  | Start play |
11h VMREWPLAY |  | Rewind and start play |
12h VMSTOP |  | Stop |
13h VMEXIT |  | Release connection without storing/erase |
20h VMREC |  | Start record |
21h VMREWREC |  | Rewind and start record |
22h VMSTORE |  | Store information and release connection |
25h VMPLAYRESA |  | Start playing of announcement |
26h VMPLAYRESI |  | Start playing of information |
27h VMPLAYRESM |  | Start playing of message |
30h VMTIM |  | Time information |
31h VMPLAYRDY |  | End of play |
32h VMRECEND |  | End of record |
33h VMREL |  | Answer on a VMEXIT or a VMSTORE |
34h VMSTORERDY |  | Answer on a VMSTORE |
35h VMRELRES |  | Answer signal to CP block form VM |
36h VMRECSIL |  | Silence detected |

Revision: F © Ericsson Enterprise 2004