BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2088
TCD for suffix dialling when authority code active (day-switched)

The command states to which trunk number category for suffix dialling during register recall to PSTN the extension belongs to when the exchange is day-switched and authority code is activated.

The trunk number category controls which numbers the extension can dial. See commands 0103 TCD-day COS/2020 TCD-day at authority code for more information.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004