BusinessPhone Communication Platform 6.0
Commands > Commands 9000...9999

## 9003
Active time for ’CBack on free’ initPBX

This command specifies the time during which a network Call Back on free mission is active in the initiating PBX.

If this timer expires the initiating PBX initiates cancellation of Call Back, the missions in initiating and supervised PBX are deleted and the Call Back has failed.

This timer can be programmed to values in steps of 5 minutes.

This timer must be programmed to the same value in every PBX which makes use of network Call Back.

The value of this timer must be at least 5 minutes less than the corresponding one in the supervised PBX (command 9005 Active time for ’CBack on free’ superPBX).

Values: 0005 (= 5 minutes) to 0855 (= 8h 55m) using the format ‘hhmm’ |  |

Initial Value: 0200 (= 2 hours) |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004