BusinessPhone Communication Platform 6.0
Commands > Commands 8000...8999

## 8201
Receiver dirno

This command is used to determine the directory number that belongs to each paging receiver.

The paging receivers are numbered sequentially (1-250).

If an extension is to have a receiver, the extension directory number has to be entered for a receiver.

If an extra receiver is required, e.g. for guests, a free directory number is entered for a receiver.

No check of entered directory numbers takes place.

If the same directory number is entered for several receivers, the receiver with the lowest serial number will be called if paging is started to the directory number.

If a directory number that matches a longer directory number is entered, paging to the longer number will not be possible.

A receiver can be marked free by erasing the directory number.

##### Valid data

1 - 4 |  | digits |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2004