BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1019
Night-switching group

The command states the night-switching group to which the trunk belongs.

Night-switching of the PABX means that incoming calls to each individual trunk are routed to a common answering position.

Night-switching of a trunk group means that incoming calls on trunks included in the group will be routed to a common answeringposition.

When the PABX is switched from day to night traffic or vice versa the trunk groups will also be switched accordingly.

Trunks can be divided into eight night-switching groups, see command group 30. Thus, there are eight possibilities of routing the incoming traffic to different answering positions.

##### Valid data

1-8 |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004