BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0xC4
Digital Link Report

Default definition: |  | ERROR + TRIG |
Used by block: |  | LS |
Category: |  | MAINTENANCE |

LS-block has got report about some error on a digital link.

Actions, when errors occur | Occurs | Ceases
Change sync. | Block new call | Disconn. ongoing call | Deblock new call
LOS, AIS, LFA, EBR | X | X | X | X
RAI | – | X | X | X
LMF, LMFR, SLIP2 | – | X | – | X
SLIP1 | X | – | – | –

- D1: Card position
- D2: Link-report error codes

- 10h: LOS, loss of signal.
- 11h: AIS, alarm indication signal.
- 12h: LFA, loss of frame synchronization.
- 13h: EBR, excessive bit-error rate.
- 14h: RAI, remote alarm indication.
- 15h: LMF, loss of multi frame synchronization (not ISDN).
- 16h: LMFR, loss of multi frame synchronization, remote side.
- 17h: CCEI, continuously CRC error information.
- 18h: SLIP1, synchronization error, when master.
- 19h: SLIP2, synchronization error, when not master.

- D3: Fault counter for current alarm (total counter)
- D4: Card position for current synchronization master, if any.

Revision: I © Ericsson Enterprise 2004