BusinessPhone Communication Platform 6.0
Commands > Commands 3000...3999

## 3831
Used Music on Hold source
(for ACD)

This command is used to assign the ACD-group to one of thirteen (0-12) possible Music On Hold sources.

Between the queue announcements, the parked caller will be connected to this programmed MOH source.

To create a Music On Hold source, see command 5403 Create music on hold.

##### Valid data

0 - 7 |  |  |
0 |  | (default) |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004