BusinessPhone Communication Platform 6.0
Commands > Commands 4000...4999

## 4315
Silent detect level VMU-HD

The detection of silence is implemented on the VMU-HD board. When silence is detected during recording of a voice message the central software will be informed and can take appropriate action.

This command defines the silence detection level. Values below are regarded as silence.

##### Valid data

-70 dBm--20 dBm |  |  |
-40 dBm |  | (default) |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004