BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0180
TCD suffix dialling-night COS

The command states to which trunk number category for suffix dialling during register recall to PSTN the extension belongs to when the exchange is night-switched. The trunk number category controls which numbers the extension can dial. see command 0104 TCD-night COS for more information.

##### Valid data

0 |  | (default) |
1-8 |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004