BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0x4D
Analog Probe Limit Exceeded

Default defintion |  | ALARM + EXTERN + ACTIVE |
Used by block: |  | RP |
Category: |  | MAINTENANCE |

An A/D converter value is out of limits or back inside the limits, depending on how the current threshold has been set. By default, warnings are generated only, when an A/D converter of type supervision detects an out-of-limits value.

- D1:
- D2: Type of A/D converter as defined in ADFUNCTION message.
- D3: Current value of given A/D converter, including controlbits,

- high byte
- Bit 7: Sign bit (0 indicates a positive value)
- Bit 6-5: 00 Not valid
- Bit 6-5: 01 Value back within limits
- Bit 6-5: 10 Value out of high limits
- Bit 6-5: 11 Value out of low limits
- Bit 4: Hundreds (0 or 1)
- Bit 3-0: Tens (0-9)

- D4: Current value of given A/D converter, including controlbits,

- low byte
- Bit 7-4: Ones (0-9)
- Bit 3-0: Tenth (0-9)

Revision: I © Ericsson Enterprise 2004