BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1414
Length detection first PTS

The command is used to state the time for detection of 1st dial tone from the connected exchange for outgoing calls.

Value = 01-20 (100-2000 ms)

The time is stated in multiples of 100 ms. (e.g. 12 = 12 * 100 = 1200 ms.)

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004