BusinessPhone Communication Platform 6.0
Dialogs

## Settings for ICCU

This frame shows the currently defined RP job settings and allows redefinition.

The following options - only one can be active at any given time - can be selected:

- Start trace from current memory address
- Clear memory and start trace

With both options a subset of flags can be set:

- From ASB
- To ASB
- From DCT
- To DCT
- From CSM
- To CSM

After the selection is complete, using the “Submit” button will set the parameters for the following traces to be started. Using “Set Default” will return everything to default values, while “Back” returns the view to the OnBoard Tracing view.

Revision: B © Ericsson Enterprise 2004