BusinessPhone Communication Platform 6.0
Commands > Commands 9000...9999

## 9103
NPI for private calling/connected line identification

The command is used to define the Number Plan Identifier (Number Plan and Type Of Number) for private (CN) calling/connected line identification.

Following combinations of NPI's are available for the private network (CN) calls:

Parameter value | Number Plan | Type Of Number | Note
10h | Private | Unknown | default
12h | Private | Regional level 1 | calling & called party with LOC * number
14h | Private | Regional level 0 (local) | calling & called party without LOC * number
20h | Unknown | Unknown | to be used e.g. when characters * and # are send as digit-information in a number

- * The LOC (LOcation Code) is the most significant part of the complete number

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004