BusinessPhone Communication Platform 6.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 90 KEYCODE

Symbols for keycodes, dummy keycodes and key types, used in the KEYCODE-message and in the OU.CALL PA.KEYASCII routine. Same symbols can be used for LED-number in the LEDRING and the LEDCTRL message.

2nd function of a key is indicated by bit7 =1 in K2ND EQU 80h; the key value. 2'nd function of KEY0= KEY0+K2ND.

Range:00h - 6Fh for keycodes

70h - 74h for keytypes

75h - 7Bh for keycodes

7Ch - 7Fh for dummy keys

80h - EFh for 2'nd function of keycodes

F0h - FFh for 2'nd function of keytypes and dummy keys

00h KEY0 |  | Keypad digit 0 |
01h KEY1 |  | 1 |
02h KEY2 |  | 2 |
03h KEY3 |  | 3 |
04h KEY4 |  | 4 |
05h KEY5 |  | 5 |
06h KEY6 |  | 6 |
07h KEY7 |  | 7 |
08h KEY8 |  | 8 |
09h KEY9 |  | 9 |
0Ah KEYSTAR |  | Keypad * |
0Bh KEYSQR |  | Keypad # |
0Ch KEYSAVE |  | SAVE |
0Dh KEYMESS |  | MESSAGE |
0Eh KEYINFO |  | INFO |
0Fh KEYPF_0 |  | Function key 0 |
0Fh KEYPICKUP |  | PICKUP (alternative name of PF_0) |
10h KEYONOFF |  | ON/OFF |
11h KEYMUTE |  | MUTE alias KEYPF_4P (DBC 2XX family) |
12h KEYCLEAR |  | CLEAR |
13h KEYR |  | R |
14h KEYPROG |  | PROG |
15h KEYDIAL |  | Speed DIAL (erase, backspace in text mode) |
16h KEYREAD |  | READ & (space in text-mode) |
17h KEYMENU |  | MENU alias KEYPF_4Q (DBC 2XX family) |
18h KEYHOLD |  | HOLD |
19h KEYTRANS |  | TRANSFER |
1Ah KEYDIV |  | DIVERSION |
1Bh KEYLINE1 |  | LINE 1 |
1Ch KEYLINE2 |  | LINE 2 |
1Dh KEYINQ |  | INQUIRY |
1Eh KEYPF_A |  | Function key A |
1Fh KEYPF_B |  | B |
20h KEYPF_C |  | C |
21h KEYPF_D |  | D |
22h KEYPF_E |  | E |
23h KEYPF_F |  | F |
24h KEYPF_G |  | G |
25h KEYPF_H |  | H |
26h KEYPF_I |  | I |
27h KEYPF_J |  | J |
28h KEYPF_K |  | K |
29h KEYPF_L |  | L |
2Ah KEYPF_M |  | M |
2Bh KEYPF_N |  | N |
2Ch KEYPF_O |  | O, 1A on DSS1 |
2Dh KEYPF_O |  | P, 1B on DSS1 |
2Eh KEYPF_O |  | Q, 1C on DSS1 |
2Fh KEYPF_O |  | R, 1D on DSS1 |
30h KEYPF_O |  | S, 1E on DSS1 |
31h KEYPF_O |  | T, 1F on DSS1 |
32h KEYPF_O |  | U, 1G on DSS1 |
33h KEYPF_O |  | V, 1H on DSS1 |
34h KEYPF_O |  | W, 1I on DSS1 |
35h KEYPF_O |  | X, 1J on DSS1 |
36h KEYPF_O |  | Y, 1K on DSS1 |
37h KEYPF_O |  | Z, 1L on DSS1 |
38h KEYPF_1 |  | Soft key 1 |
39h KEYPF_2 |  | 2 |
3Ah KEYPF_3 |  | 3 |
3Bh KEYPF_4 |  | 4 |
3Ch KEYENTER |  | ENTER |
3Dh KEYCONF |  | CONFERENCE |
3EH KEYMINUS |  | Volume – |
3FH KEYPLUS |  | Volume + |
40h KEYPF_1M |  | Function keys for DSS1 (cont.) 1M on DSS1 |
41h KEYPF_1N |  | 1N on DSS1 |
42h KEYPF_1O |  | 1O on DSS1 |
43h KEYPF_1P |  | 1P on DSS1 |
44h KEYPF_1Q |  | 1Q on DSS1 |
45h KEYPF_2A |  | Function keys for DSS 2 2A on DSS2 |
46h KEYPF_2B |  | 2B on DSS2 |
47h KEYPF_2C |  | 2C on DSS2 |
48h KEYPF_2D |  | 2D on DSS2 |
49h KEYPF_2E |  | 2E on DSS2 |
4Ah KEYPF_2F |  | 2F on DSS2 |
4Bh KEYPF_2G |  | 2G on DSS2 |
4Ch KEYPF_2H |  | 2H on DSS2 |
4Dh KEYPF_2I |  | 2I on DSS2 |
4Eh KEYPF_2J |  | 2J on DSS2 |
4Fh KEYPF_2K |  | 2K on DSS2 |
50h KEYPF_2L |  | 2L on DSS2 |
51h KEYPF_2M |  | 2M on DSS2 |
52h KEYPF_2N |  | 2N on DSS2 |
53h KEYPF_2O |  | 2O on DSS2 |
54h KEYPF_2P |  | 2P on DSS2 |
55h KEYPF_2Q |  | 2Q on DSS2 |
56h KEYPF_3A |  | 3A on DSS3 |
57h KEYPF_3B |  | 3B on DSS3 |
58h KEYPF_3C |  | 3C on DSS3 |
59h KEYPF_3D |  | 3D on DSS3 |
5Ah KEYPF_3E |  | 3E on DSS3 |
5Bh KEYPF_3F |  | 3F on DSS3 |
5Ch KEYPF_3G |  | 3G on DSS3 |
5Dh KEYPF_3H |  | 3H on DSS3 |
5Eh KEYPF_3I |  | 3I on DSS3 |
5Fh KEYPF_3J |  | 3J on DSS3 |
60h KEYPF_3K |  | 3K on DSS3 |
61h KEYPF_3L |  | 3L on DSS3 |
62h KEYPF_3M |  | 3M on DSS3 |
63h KEYPF_3N |  | 3N on DSS3 |
64h KEYPF_3O |  | 3O on DSS3 |
65h KEYPF_3P |  | 3P on DSS3 |
66h KEYPF_3Q |  | 3Q on DSS3 |
67h KEYPF_4A |  | 4A on DSS4 |
68h KEYPF_4B |  | 4B on DSS4 |
69h KEYPF_4C |  | 4C on DSS4 |
6Ah KEYPF_4D |  | 4D on DSS4 |
6Bh KEYPF_4E |  | 4E on DSS4 |
6Ch KEYPF_4F |  | 4F on DSS4 |
6Dh KEYPF_4G |  | 4G on DSS4 |
6Eh KEYPF_4H |  | 4H on DSS4 |
6FH KEY2ND |  | 2'nd function key |
70h KEYS.INV |  | Invalid as key-code |
71h KEYS.DIGIT |  | Keypad (digits and *#) |
72h KEYS.LINE |  | Line-keys (3-line) |
73h KEYS.PGM |  | Programmable |
74h KEYS.SOFT |  | Soft function-keys |
75h KEYPF_4I |  | Function key 4I on DSS4 |
76h KEYPF_4J |  | 4J on DSS4 |
77h KEYPF_4K |  | 4K on DSS4 |
78h KEYPF_4L |  | 4L on DSS4 |
79h KEYPF_4M |  | 4M on DSS4 |
7Ah KEYPF_4N |  | 4N on DSS4 |
7Bh KEYPF_4O |  | 4O on DSS4 |
7Ch KEYD.CTI |  | CTI. A certain number is requested without knowing the key number where this function is located. |
7Dh KEYD.ENDBLOCK |  | Transfer one or more numbers or parts of numbers in one message. |
7Eh KEYS.WAITDT |  | Wait for second dial tone |
7Fh KEYS.INQSUP |  | Inquiry in superior exchange |
80h KEY_ALBUT |  | RP Keycode for alarm button |

Revision: F © Ericsson Enterprise 2004