BusinessPhone Communication Platform 6.0
Dialogs

## CPU settings

Error Messages:

- Send error messages to printer: This parameter enables or disables the printer that is connected to the ICCU2. Enable this parameter if the support specialist requires a hard copy of the service messages. For connecting the printer to the IC‑CU2, see board description of IC‑CU2. The messages are printed in order of appearance. Service messages that appeared before the printer was enabled will not be printed. Press the on-line button on the printer at least twice, so that the printer is on-line. Disable this parameter before disconnecting or switching off the printer. Otherwise the operation of the test and maintenance module will be slowed down.
- Overwrite error messages: This parameter enables or disables the overwrite option of service messages. If enabled, the latest report error may overwrite a previous logged error. If so, only the time is updated. The selection is stored in non-volatile memory.

Logging:

- Send event logging to BMS-DECT: This parameter is not intended for normal installation and maintenance purposes. If the Technical Assistance Centre needs some logs of the system, you can activate it by enabling this parameter.
- Logfile name: Name of the event logging file.

#### Actions

Transfer to ICCU2 |  | To start the selected process. |

Revision: B © Ericsson Enterprise 2004