BusinessPhone Communication Platform 6.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## B4 CONPTYNUM

1 CONPTYREQ |  | RP Request of number |
2 CONPTYACK |  | RP accepted |
3 CONPTYNAK |  | RP rejected |
4 CONPIDACK |  | Calling or connected (answering) number and name information |
5 CONPIDDIV |  | Calling or connected (answering) number and name information, diverting number and name information |
6 CONPTFRREQ |  | Request for 'new' calling/connected identity after call transfer |
7 CONPIDTFR |  | Sending of 'new' calling/connected number and name after call transfer |
8 CONPIDRER |  | Calling or connected (answering) number and name information, rerouting number and name information |

Revision: F © Ericsson Enterprise 2004