BusinessPhone Communication Platform 6.0
Commands > Commands 9000...9999

## 9102
Call back allowed ?

The command states whether automatic call back may be set up to the private network access code.

Following command for the route will be ignored: 3302 Callback allowed?.

##### Valid data

Yes |  |  |
No |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004