BusinessPhone Communication Platform 6.0
Commands > Commands 5000...5999

## 5434
Create Mobile Access

This directory number is used as access point, which reroutes calls from a Mobile Extension to its internal directory number and calls to a Mobile Extension to its public external number.

ASB 150 02 permits a maximum of 16 mobile access numbers.

##### Valid data

4 digits |  | (0-9,*,#,-) |

Note

Command 5534 Delete Mobile Access is used to delete the directory number for this facility. Command 5634 Alter Mobile Access is used to alter the directory number for this facility.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004