BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0107
Break-in allowed?

On a call to a busy extension it may be possible (permitted) to intrude (break in) on the ongoing call, i.e. effect intrusion.

With this command other user may have access to intrude on a call in which the extension is in speech.

Only those extensions (PABX-operators) whose facility category permits intrusion are allowed to initiate this facility. See command 3004 Intrusion.

##### Valid data

Yes |  | (default) |
No |  |  |

Note

When this command, for an analogue extension, is set to NO, outgoing ISDN calls will have bearer capabilities changed to 3.1 kHz audio. This may be used if a fax or modem is connected.

In some ISDN networks this may not be allowed.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004