BusinessPhone Communication Platform 6.0
Commands > Commands 8000...8999

## 8304
Reminder answer anno

When an extension or PBX-operator answers a reminder, a voice message can be played as acknowledgement. This command determines the voice message to be played. The directory number for the voice message is created via command 5408 Create voice answer. Command 4701 Reference number for voice answer determines the voice references to be included in the voice message. The voice references are recorded with a system telephone in system programming mode (see command group 4400).

Command 3069 Reminder ordering is utilised to determine authorisation for use of the reminder facility.

##### Valid data

Voice answer reference directory number |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2004