BusinessPhone Communication Platform 6.0
Commands > Commands 3000...3999

## 3502
Exit position of PBX group

This command defines the exit position of the PBX group.

An internal directory number as well as a CN destination will be accepted. Valid internal directory numbers are:

- extension
- operator
- fictive number
- voice anser reference number
- common short number
- common mailbox
- ACD group directory number
- PBX group.
- By default, no number is defined.

The exit position is erased by overwriting it with blanks. If no exit position is defined, an external call will be rerouted to the reroute position of the incoming trunk (see command 1103, 1104) and an internal call will be disconnected.

##### Valid data

0 |  | (digits) |
1-8 |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004