BusinessPhone Communication Platform 6.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 56 RPJOBANSW

01h RPJCSUM |  | Compute PROM checksum |
01h RPJACSUM |  |  |
81h RPJACSUM_ERR |  |  |
02h RPJLED |  | Control LED's on board front |
02h RPJALED |  |  |
82h RPJALED_ERR |  |  |
03h RPJBREV |  | Asks for board revision |
03h RPJABREV |  |  |
83h RPJABREV_ERR |  |  |
05h RPJPRNO1 |  | Asks for product number of PROM1 |
04h RPJAPRNO1S |  |  |
05h RPJAPRNO1P |  |  |
85h RPJAPRNO1_ERR |  |  |
07h RPJPRNO2 |  | Asks for product number of PROM2 |
06h RPJAPRNO2S |  |  |
07h RPJAPRNO2P |  |  |
87h RPJAPRNO2_ERR |  |  |
09h RPJPRNO3 |  | Asks for product number of PROM3 |
08h RPJAPRNO3S |  |  |
09h RPJAPRNO3P |  |  |
89h RPJAPRNO3_ERR |  |  |
0Ah RPJCADR |  | Asks for card address (from port) |
0Ah RPJACADR |  |  |
8Ah RPJACADR_ERR |  |  |
0Bh RPJTRACE |  | To control the trace function |
0Bh RPJATRACE |  |  |
8Bh RPJATRACE_ERR |  |  |
0Eh RPJCROF |  | Asks for product number of card (ROF...) |
0Dh RPJACROFS |  |  |
0Eh RPJACROFP |  |  |
8Eh RPJAROF_ERR |  |  |
0Fh RPJPERTEST |  | Asks for periodic test |
0Fh RPJAPERTEST |  |  |
8Fh RPJAPERTEST_ERR |  |  |

Revision: F © Ericsson Enterprise 2004