BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2147
GW TTL enabled

For each of the in command 2145 GW RAS transport address defined GWs it has to be specified if the GW is capable to support the TimeToLive mechanisms (light weight registrations) as specified in H.323.

By default it is enabled.

##### Valid data

0 |  | Time to live mechanism disabled |
1 |  | Time to live mechanism enabled (default) |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004