BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0162
Terminal type

This command can be used to define the terminal type connected to an analogue extension interface. If the default value is selected, the extension is used as ordinary analogue terminal.

##### Valid data

0 (default) |  |  |
1 |  | general, 3.1kHz audio, orig.non ISDN |
2 |  | group 3 fax, 3.1kHz audio, orig.non ISDN |
3 |  | modem, 3.1kHz audio, orig.non ISDN |
4 |  | fax, 3.1kHz audio, orig.non ISDN |
5 |  | mobile extension |

Additional information for option 3 (modem) : Using this option in combination with ISDN-lines and analogue extensions leads to releasing of DTMF-registers after receiving call proceeding.

Note

This option must not be used in combination with LCR !

If the extension is configured as FAX EXTENSION (option 2 or 4) some restrictions in the settings of the following facilities have to be concerned.

#### Extension related facilities

- conference
- call back
- break-in
- camp-on
- diversion
- follow me

#### Trunk related facilities

- reroute position
- voice announcement

Additional information for option 5 (mobile extension):

- If an analog extension (defined as a Mobile Extension) orders an internal or a CN callback, the duration of callback ringing time is set fixed to 30 seconds - even if command 9006 (Maximal ringing time at the initiating extension for Call Back calls) is set to another value.
- Time within the user is requested to lift the handset in case of a call set up done by the CTI application is set fixed to 16 seconds.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004