BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1951
Interface type

This command is used to specify the type of Basic Access connection mode. At connection to S-interface user mode is valid. At connection to T-interface network mode is valid. At connection to T-interface network mode (Q-reference point) is valid.

Note

The selected type of connection has to correspond to DIP switching of interface type on BTU-B board.

##### Valid data

USER (-S) |  |  |
NETWORK (-T) |  | Default |
NETWORK (-Q) |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004