BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1022
Voice info to trunk allowed?

The command is used to state whether voice information for incoming trunk traffic shall be given to an extension possessing the voice information function.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004