BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1613
Relative sending level during DTMF

The command is used to state the relative transmission level (Lo) in the analog interface on the external line in case of register signaling with DTMF.

##### Valid data

12 - +6dBr |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004