BusinessPhone Communication Platform 6.0
Dialogs

## DECT System

BMS integrates the ICCU2 related parts of CSM. Because ICCU2 uses the GAP protocol, only this functionality is supported. As most users are familiar with CSM, an overview of its functionality is given as well as a reference to locate the integrated features within BMS.

Note

The DECT menu is only available if you are connected to a DECT system.

### Connection to the DECT System

- Connect to BusinessPhone (go online)
- Click on “Dect” and select “Activate DECT”
- Check the progress. The message “Activating DECT connection...” appears on the screen.
- As soon as BMS responds with “The DECT system is now available for OAM!” The DECT system is now connected.

### DECT context menu

- Click on “Dect...” in the menu tree to open the context menu with the following items:

- (Re)Initialize - Reinitialization of a system. The system data is deleted and a reset command is issued.
- Reset system - Resets the system.
- Backup - Saves a copy of the system configuration in case of emergency.
- Restore - Sends a set of stored data to the system.
- System Configuration - To change various system parameters that had been set during (re)initialization.
- Reset alarm relay - To reset the Alarm Relay LED on the ICCU-board.
- Create Report - The service report dumps some interesting data to a file.
- Deactivate DECT - To shut down the DECT system.

### DECT - Boards

- In the Configuration directory tree, click on the DECT submenu “Boards” to open the context menu. Only one item appears: “Properties”.
- Click on “Properties” to open the Radio Exchange dialog. This dialog gives a hardware overview of the system. See also Radio Exchange.

### DECT - Base Stations

- In the directory tree on the left side, click on the DECT submenu “Base Stations” to open the context menu with the two menu items “Properties” and “Download SW”.
- Click on “Properties” to open the Base Station dialog. This dialog gives an overview of the base stations of the system. See also Base Stations.

- or

- Click on “Download SW” to open the Base Station Download dialog. In this dialog, you can upload a new software release to a certain number of Base Stations. See also Base Station Download.

### DECT - Cordless

- In the Configuration directory tree on the left side, click on the DECT submenu “Cordless” to open the context menu. Only one item appears: “Properties”.
- Click on “Properties” to open the Cordless Phones dialog. This dialog gives an overview of the Cordless phones used in the system.

For more information, please refer to the sections Cordless Phones and Subscription.

### DECT - Information

- In the Configuration directory tree, click on the DECT submenu “Information” to open the context menu. The Information menu comprises the following menu items:

- Call events - See Call Events
- Service messages - See Service Messages
- Statistic overview - See Statistics Overview
- Reset history - See Reset History

Revision: B © Ericsson Enterprise 2004