BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0x76
RP DSLAC Error

Default definition: |  | ERROR |
Used by block: |  | BTU, ELU-A |
Category: |  | DESIGNER |

The DSLAC is tested at restart and during traffic, by reading back written data. A warning message is sent in case that read data is not the same as the written data.

- D1: Individual number
- D2: Faulty DSLAC command
- D3: Undefined
- D4: Undefined

Revision: I © Ericsson Enterprise 2004