BusinessPhone Communication Platform 6.0
Dialogs

## Settings for BTUB

This frame shows the currently defined RP job settings and allows redefinition.

The following options - only one can be active at any given time - can be selected:

- Start trace from current memory address
- Clear memory and start trace
- Start trace on BRA link individual:
  The link number can be selected using the

- BRA link selector

- Start trace on code:
  The code (Infocode) can be entered either as numerical values or via its named abbreviation.
- Start trace & Tracestop on warning:
  A code triplet has to be entered.
- Clear memory & Start ISDN trace
- Start ISDN layer 2 trace

After the selection is complete, using the “Submit” button will set the parameters for the following traces to be started. Using “Set Default” will return everything to default values, while “Back” returns the view to the OnBoard Tracing view.

Revision: B © Ericsson Enterprise 2004