BusinessPhone Communication Platform 6.0
Commands > Commands 3000...3999

## 3822
Call code after terminated call

This command is used to state whether the ACD-operator must specify a call code after a terminated call. Call codes can be used after the postprocessing (clerical) program and, thus, statistics of which type of facility is used most frequently is shown.

If YES, then the range of values for command 3820 Postprocessing (clerical) time is set to 5-255 sec. If less than 5 seconds are programmed, the value is automatically changed to 5.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004