BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0124
Call waiting tone for non system instruments?

This command states whether or not an analogue, cordless or IP extension is allowed to receive a call-waiting tone.

Only non system instruments are concerned, as digital extensions use the tone-ringer to announce call waiting.

Note

Mobile extensions never get a call waiting tone.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004