BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0xBA
E2DATA Conversion Error

Default definition: |  | ALARM + EXTERN + ACTIVE |
Used by block: |  | CE |
Category: |  | MAINTENANCE |

The warning is used, when either E2NAK or TIMEOUT1 is received as response to an E2-message during a common restart.

- D1: Card position
- D2: Individual number
- D3: State
- D4: 0

Revision: I © Ericsson Enterprise 2004