BusinessPhone Communication Platform 6.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 47 CPJOB

000h CPJUNDEF |  | Job undefined |
010h CPJPRODNUM |  | Ask of part of CXC-number |
011h CPJPRODNUMANSW |  | Answer |
020h CPJSETFORMAT |  | Set communication format |
030h CPJREAD |  | Read CP-memory |
031h CPJREADI |  | Read CP-memory, indirect |
032h CPJREADIND |  | Read CP-memory, individual ram |
03Fh CPJREADANSW |  | Answer |
040h CPJTESTSTART |  | RP Setup message for test |
041h CPJTESTLOG |  | RP Setup message for starting log |
042h CPJTESTEND |  | RP Test disable |
043h CPJTESTLOGMPD |  | RP Setup message for starting log for MPD |
050h CPJTESTBOARD |  | RP Identification of test board |
0E0h CPJOMPCCOM |  | Command to PC handler in OM-block |
0F0h CPJMESS |  | A short message packed and sent in complete form with one CPJOB-message |
0F1h CPJMESSFST |  | First part of a long, packed, message |
0F2h CPJMESSMID |  | Middle parts, of a packed message |
0F3h CPJMESSLST |  | Last part of a packed message |

Revision: F © Ericsson Enterprise 2004