BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1947
Handling of call collisions

This command states the side (A or B) of the network which is assigned to this interface for the handling of call collisions.

In symmetrical arrangements call collisions can ocurr when both sides simultaneously transfer a SETUP message indicating the same B_channel.

In order to minimize the chances of call collisions, one side of the connection (side A) assign the lowest available channel number and the other side of the connection (side B) assigns the highest.

##### Valid data

0 |  | Side B |
1 |  | Side A |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004