BusinessPhone Communication Platform 6.0
Commands > Commands 4000...4999

## 4437
Voice Message Prompts - Forward a message

Minimum required authority level from telephone: 1

The following voice prompts are are described for each voice announcement.

voice prompts | used for | predefined text
4437-0 | send, forward | “You are not allowed to send a message, please contact your system administrator”
4437-1 | send | “After the tone, please record your message, - To finish recording, press HASH (#)”.
4437-2 | send | “Recording time exceeded. Your message has not been recorded”.
4437-3 | send | “Send menu: - To record the message again, press ONE (1), - To listen to it, press TWO (2), - To send it, press THREE (3), - To go back to the main menu, press ZERO (0)”.
4437-4 | send, forward | “Please enter the mailbox number”.
4437-5 | send, forward | “This number does not exist”.
4437-6 | send, forward | “This number is not allowed to receive messages”.
4437-7 | send, forward | “The number is”.
4437-8 | send, forward | “If this is correct, press STAR (*), - To change the number, press HASH (#)”.
4437-9 | send, forward | “Your message could not be sent”.
4437-10 | send, forward | “Your message has been sent”.
4437-11 | send | “To send this message to another number, press ONE (1), - To go back to the main menu, press Oh (0)”.
4437-12 | forward | Forwarded message from...(+ number of MBX sender)
4437-13 | send | Your message was not recorded.

Revision: E © Ericsson Enterprise 2004