BusinessPhone Communication Platform 6.0
Start of operation ASB 150 02

## Prerequisites

- The skilled technician should be familiar with the PBX in terms of location of the switches on the boards and the settings by BMS.
- The system shall already be mounted.
  Presently two different cabinets are available which shall be mounted in accordance with:

- “Installation Instruction BP 250” (1531‑BDV 113 08 Uen) and
- “Installation Instruction BP 128i” (1531‑BDV 101 06 Uen) and
- “Installation Instruction BP 50” (1531‑BDVBS 101 05 Uen).

- A PC installed with the maintenance program:

- BMS (BusinessPhone Management Suite, FASBS 102 213)

- To connect the maintenance PC with the system, use cord set TSR 902 0448/1.

Revision: K © Ericsson Enterprise 2004