BusinessPhone Communication Platform 6.0
Dialogs

## Common Bell

You can define a common bell extension for a system. This way, all extensions within a system can pick up a call to the common bell number.

To access the dialog, open the “Features” menu in the configuration directory tree and click on the “Common Bell” submenu.

The dialog consists of three fields:

5629 |  | Pickup code for common bell

6501 |  | Directory name

6901 |  | Common bell extension

For more information about a field, click on the command link in brackets. See also facility description Common Bell (151/15534-ASB 150 02 Uen).

### Creating a common bell extension

- Enter the code for the common bell feature in the first field of the dialog or accept the default code that is displayed when you open the dialog.
- Enter the directory name of the extension.
- Enter the number of the common bell extension.

Note

If the entered extension number does not exist or causes a conflict with an existing directory number, an error message will appear. Read the error message carefully to solve the problem.

- Click on Submit. If the changes have been successful, the dialog shows the number of the common bell extension in the last field.

#### Actions

Submit |  | To send the settings to the system. |
Reload |  | To show the current system settings. |

Revision: B © Ericsson Enterprise 2004