BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1717
Answer signal?

The command is used to state whether the line signal “answer” shall be received (exists) at outgoing calls.

Note

Ascertain that the signal is included in the selected line signal scheme.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004