BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0123
Repeated call diversion?

Diversion on no reply means that incoming calls to an extension will be diverted to a predetermined divertee (answer) position unless they are answered within a predetermined time. See command 0110 Diversion on no reply at internal calls? for more information.

The system offers extension supervision with call pickup with the help of programmable keys. See command 0301 Key function.

Call diversion on no reply is normally not permitted if the call is already diverted. In cases where it is not possible to utilise programmable keys for call diversion (interception) it may nevertheless be desirable with repeated call diversion.

This command is used to state whether calls to the extension may be diverted on no reply despite the fact that they have already been diverted.

If several extensions are assigned this possibility, this may result in long diversion chains.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004