BusinessPhone Communication Platform 6.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 78 UPDCARD

1 SUCARDDEL |  | E2-data for a removed card will be deleted |
2 SUCARDINS |  | E2BASE areas for a new card are installed |
3 SUSHDWNREQ |  | Request shutdown of card |
4 SUSHDWNEXEC |  | Execute card shutdown |
5 SUSHDWNACK |  | Acknowledge to SUSHDWNREQ and SUSHDWNEXEC |
6 SUCARDDELACK |  | Acknowledge to SUCARDDEL |
7 SUSHDWNDELACK |  | Acknowledge to SUSHDWNDEL |
8 SUSHDWNINS |  | Shutdown of VMU-HD unit |
9 SUSHDWNAUT |  | Automatic restart of VMU-HD unit |

Revision: F © Ericsson Enterprise 2004