BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0110
Diversion on no reply at internal calls?

The command defines if a diversion on no-reply on an internal call should be done.

If the extension is a master and member of a tandem configuration the command data shall be copied to the slave and blocked for the slave's further use.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: 0

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004