BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1911
Network signalling protocol

The command is used to define the network signalling protocol for the current ISDN-link.

Available network signalling tables for T-reference point, DSS1, are:

1. Australia
2. ETSI
3. Belgium
4. Italy
5. Netherlands
6. Sweden
7. Spain
9. Finland
10. Denmark
11. New Zealand
12. Swissnet
13. Bezeq
14. Greece
15. Brazil

Available network signaling tables for Q-reference point, QSIG, are:

130 - ETSI/ECMA

131 - ETSI/ISO

Used initial values:

DSS1...ETSI network signalling

QSIG....ETSI/ECMA network signalling

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004