BusinessPhone Communication Platform 6.0
Facilities

## Austria – Support Of Packet Mode Terminals

## Definition

This document should be seen as a supplementary document to the ISDN Facilities Description (268/155 34-ASB 150 02 Uen) which focuses especially on the support of packet-mode terminals (based on X.25/X.31) for the Austrian Market.

ASB 150 02 supports two different kinds of transfer modes for the bearer services on the S-Interface:

- Circuit mode
- Packet mode

For the bearer service packet mode ASB 150 02 supports a maximum of 9.6 kbs through the D‑channel.

The behaviour of the circuit-mode calls and packet- mode calls is different with regard to switching and routing within ASB 150 02.

## Use

The support of packet-mode connections on the S‑Interface is used for terminals (e.g. Point-Of-Sales Terminals; POS) which do not support circuit-mode data calls.

This functionality provides the possibility to save a dedicated Basic Access (BA) only for POS traffic, which has been done in most cases more or less independently from the ASB 150 02 system.

## Operation

Packet-mode terminals will be connected to the S‑Interface in the same way as all the other ISDN equipment, such as ISDN telephones or PC-cards.

ASB 150 02 supports packet-mode terminals which send X.25 packets over an ISDN BA using the Service Access Point Identifier (SAPI)* value equal to 16 and a Terminal Endpoint Identifier (TEI)* value in the non-automatic range (0-63) (*: address mechanism in Layer 2).

Compared to the circuit-mode calls which can be routed through the switch to almost every directory number in the system, the routing of packet-mode calls is defined by programming from one data link on one S-Interface to another data link on a T‑Interface, both located on the same BTU-B / MFU board (see picture below).

The contents of the X.25 packets are not examined by ASB 150 02, they are routed unchanged between the defined data links.

ISDN Terminal equipment (TE) supporting the bearer service circuit mode or packet mode can be mixed on the S-Interface and also be used independently, due to the different SAPI (circuit mode=0, packet mode=16).

Each packet mode terminal must be subscribed to the network operator, to get its own assigned TEI value (for SAPI 16) and its own national significant number which can be but may not be the same as used for the circuit mode calls. Both assignments are hereby related to the BA used for the packet-mode traffic.

The assigned TEI from the network operator which has to be stored in ASB 150 02 at the T-Interface can be but need not be the same as stored on the packet-mode terminal due to fact that ASB 150 02 is able to perform a TEI conversion.

Most of the packet mode terminal suppliers maintain their products (e.g for software updates) by setting up a packet-mode communication to the terminal, but there exist also products which will be maintained via a circuit-mode call. In the latter case it is necessary that these terminals also have an internal directory number assigned in order to be reached.

### Read out statistics via BMS

BMS provides statistics about the packet mode communication link(s). The received information is available for each BTU-B/MFU card, which has assigned packet-mode communication links.

View the statistics under:

- MAINTENANCE-> SYSTEM-> PMC supervision

Content of the statistics:

- connected interfaces, A- and B-side of packet-mode connections (If),
- used TEI values (TEI),
- state of data link (State),
- number of X.25 packets that are transmitted towards a link, A-/B-side, (Tx),
- number of X.25 packets that are discarded (Discard)

## Capacity

- A maximum of eight packet-mode communication links can be used per S/T-interface.
- A maximum of eight TEs can be connected to the S‑Interface, whereby each of them may use 2 logical links (circuit mode and packet mode).
- A maximum of 32 packet-mode communication can be to established per BTU-B (4 T to S links) and 16 per MFU (2 T to S links) or a sub-equipped BTU-B.
- A maximum of 3 BTU-B / MFU boards can be programmed for packet-mode handling.
- The maximum size of un-segmented X.25 packets is 260 octets.

Note

There exist some POS terminal suppliers, which provide the functionality to connect only one POS terminal to the S-Interface and all further POS terminals are connected in a kind of internal bus configuration to the first POS terminal. This kind of solution has the advantage that only one X.25 terminal has to be subscribed to the network operator as well as only one packet mode communication link will be occupied in the system.

## Limitations

- A maximum of 2 TEs per S-interface can be powered via the BTU-B / MFU, the others need an own dedicated power supply.
- Only TEI values in the non-automatic range (0-63) can be used.
- Routing can only be done between packet mode communication links on the same BTU-B / MFU board.

## Programming

The following commands are only accessible via BMS:

Note

The selected type of connection (T‑interface or S-interface) has to correspond to DIP-switching of the interface type on the BTU-B / MFU board. If the DIP switching does not correspond to the selected type of interface, a warning will be generated (see Installation Instructions, 1531-ASB 150 02 Uen).

Note

The following settings have to be performed if only packet-mode terminals are connected to the S-Interface.

If there exists a mixed configuration between packet-mode and circuit-mode terminals please refer to the programming mentioned in the ISDN Facilities description (268/155 34-ASB 150 02 Uen).

1951 |  | Basic Access mode

1952 |  | User according to

1953 |  | Type of bus

1980 |  | Packet Mode Communication (PMC) links

## Equipment

### Hardware, Software

- BTU-B/MFU
- The feature is supported by ASB 150 02 R11 or higher system releases.

### Licensing

In order to have access to the feature, the proper licensing concept has to be used, see Facility Description – General (155 34-ASB 150 02 Uen), chapter ASB150 02 Licensing.

Revision: D © Ericsson Enterprise 2004