BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2074
Local private code for composing A or B number

This command defines the local private code which is used to compose the CN calling or connected number. It is used to prefix the internal directory number.

Example:

directory number: |  | 1333 |
LPC (command 2074): |  | 42 |
removed digits (command 2073 Removed digits for composing A or B number): |  | 1 |
Own location code(command 5431 Create Own Location Code): |  | 800 |
TON (command 9103 NPI for private calling/connected line identification): |  | regional level 1 |

In this case the sent calling or connected CN number is 80042333.

Note

The maximum length of sent calling or connected number is 8 digits. If the composed number is longer, then the last digits will be cut.

value: 0 to 4 digits.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004