BusinessPhone Communication Platform 6.0
Commands > Commands 3000...3999

## 3509
No Trunk Reroute

This command defines if an external call to a busy PBX group (all members are busy) shell be rerouted to the reroute position of the incoming trunk or not, if the PBX group has no defined exit position.

0 The incoming trunk will reroute the call to its reroute position

1 The incoming trunk will disconnect the call and send a busy tone

The default value for this command is 0

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004