BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0177
Initiate callback in corporate network?

The command defines if an extension is allowed to request a call back from an extension within the corporate network.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004